|  |  |
| --- | --- |
| System | Track Controller |
| Use Case | Pass Non-relevant Messages |
| Actors | Track Controller, CTC Office, Track Model |
| Description | * The CTC Office is trying to send messages to other system components. * The data sent are the: * General message command (int value) * String containing general message * The Track Model is trying to send or relay messages to or for other system components. * The data sent are the: * General message Command (int value) * String containing general message |

|  |  |
| --- | --- |
| System | Track Controller |
| Stimulus | The CTC Office establishes an Ethernet connection with the track controller and sends transmission data containing the general message command (int value). |
| Response | Track Controller packages and sends general message command and string containing general message to the Track Model. |
| Comments | There is a not a preferred frequency for which general messages to be relayed. |

|  |  |
| --- | --- |
| System | Track Controller |
| Stimulus | The Track Model establishes a connection with the track controller and sends transmission data containing the general message command (int value). |
| Response | Track Controller packages and sends general message command and string containing general message to the CTC Office. |
| Comments | There is a not a preferred frequency for which general messages to be relayed. |