|  |  |
| --- | --- |
| System | Track Controller |
| Use Case | Pass Authority |
| Actors | Track Controller, CTC Office, Track Model |
| Description | * The CTC Office transmits the track authority for a train to the Track Controller. * The data sent are the: * The track authority. * The name of the train. * The Track Controller transmits the track authority for a train to the Track Model. * The data sent are the: * The track authority. * The name of the train. |

|  |  |
| --- | --- |
| System | Track Controller |
| Stimulus | The CTC Office establishes an Ethernet connection with the track controller and transmits the track authority. |
| Response | The track controller transmits the track authority to the Track Model. |
| Comments | There is a not a preferred frequency for which track authority is received and sent. |